<?xml version="1.0" encoding="UTF-8"?>

<language_definitions>
<!--
  <language processor="CR16A/B"
            endian="little"
            size="16"
            variant="default"
            version="1.1"
            slafile="CR16B.sla"
            processorspec="CR16.pspec"
            manualindexfile="../manuals/CR16.idx"
            id="CR16AB:LE:16:default">
    <description>National Semiconductor's CompactRISC CR16A/B little endian</description>
    <compiler name="default" spec="CR16.cspec" id="default"/>
  </language>
-->
  <language processor="CR16C"
            endian="little"
            size="16"
            variant="default"
            version="1.1"
            slafile="CR16C.sla"
            processorspec="CR16.pspec"
            manualindexfile="../manuals/CR16.idx"
            id="CR16C:LE:16:default">
    <description>National Semiconductor's CompactRISC CR16C little endian</description>
    <compiler name="default" spec="CR16.cspec" id="default"/>
  </language>
</language_definitions>
